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2MP CAM(摄像头)
[image: ]基本描述/General Description 
合肥晟泰克车载摄像头采用高动态车规图像传感器,配合主流串行传输芯片,使得该模组具有高可靠性能, 该模组具有广泛适用性，能适配不同的SOC 平台。
Vehicle camera module of Hefei Softec adopts high dynamic vehicle gauge image sensor, with mainstream serial transmission chip, making the module has high reliability performance, the module has a wide range of applicability, can be adapted to different SOC platforms.
[image: ]特点/Features
● 车规高性能 /High Performance Automotive Grade;
● 传感器高动态范围/Advanced On−Sensor HDR;
● 支持多相机同步/Multi−Camera Synchronization Support;
● 多款不同焦距镜头可选/Support different focal length lens;
[image: ]应用/Application
· 行车记录仪/ Dashcam Camera
· 高级辅助驾驶和视觉融合/ADAS + Viewing Fusion
· 高动态应用/High Dynamic Range Imaging
[image: ]硬件框图/Hardware block diagram
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[image: ]关键参数/ KEY PARAMETERS
	序号
	Sensor参数
	OV OX02D10

	1
	Active Pixels(有效像素)
	2MP

	2
	Image Size(图像尺寸)
	1/2.44-inch CMOS

	3
	Shutter Type(曝光模式)
	Rolling Shutter 卷帘快门

	4
	Output Pixels(输出像素)
	1920*1080

	5
	Pixel Size(像素尺寸)
	[bookmark: _GoBack]2.9um*2.9um

	6
	ISP参数
	FH8332

	7
	Frame Rate(帧率)
	30fps

	8
	Output data(输出信号格式)
	YUV422

	9
	Lens参数
	CD316(宇瞳)

	10
	Lens Type(镜头结构)
	4G+IR

	11
	F/No.
	2.0±5%

	12
	EFL
	3.0±5%

	13
	F.O.V(Horizontal/Vertical)
	[bookmark: OLE_LINK3][bookmark: OLE_LINK2]H:122.77°±3°
V:62.05°±3°

	14
	OP Distortion(OP畸变)
	-76.6%±5%

	15
	Relative Illumination(相对照度)
	44.9%±5%

	16
	Focusing Distance(调焦距离，物距)
	500mm(按应用的物距)

	17
	Depth of Field(景深范围)
	40mm-infinity

	18
	整体模组
	参数

	19
	Dimensions(尺寸)
	L: 28mm, W:25mm, H:47mm

	20
	Weight(重量)
	＜50g

	21
	Connector(连接器)
	电连-818032090

	22
	Serializer(串行器)
	MAXIM MAX96717F

	23
	Power Supply(工作电压)
	7-9V

	24
	Current(工作电流)
	＜100mA

	25
	Camera Interface(摄像头接口)
	LVDS

	26
	Optical Axis Precision(光轴精度)
	X:±5 Pixel,Y: ±5 Pixel;

	27
	Startup Time(启动时间)
	≤500ms

	28
	Operating temperature(工作温度)
	-40℃~85℃

	29
	Storage temperature(存储温度)
	-40℃~95℃

	30
	IP Grade(防护等级)
	模组本体IP52

	31
	MTF(清晰度)
	中心视场：MTF50P≥0.55
0.7视场：MTF50P≥0.38

	32
	Low Light(最低照度)
	1Lux

	33
	SNR(信噪比)
	41.8dB

	34
	HDR Range(动态范围)
	long HCG: 73 dB
stagger HDR: 97 dB



附件Ⅰ：摄像头本体尺寸示意图(单位：mm)
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