[image: ][image: 未标题-1.png]STK-HD-CAM-OX08D10-SPEC
8MP CAM(前视摄像头)
[image: ]基本描述/General Description 
合肥晟泰克车载摄像头采用高动态车规图像传感器,配合主流串行传输芯片,使得该模组具有高可靠性能, 该模组具有广泛适用性，能适配不同的SOC 平台。
Vehicle camera module of Hefei Softec adopts high dynamic vehicle gauge image sensor, with mainstream serial transmission chip, making the module has high reliability performance, the module has a wide range of applicability, can be adapted to different SOC platforms.
[image: ]特点/Features
● 车规高性能 /High Performance Automotive Grade;
● 传感器高动态范围/Advanced On−Sensor HDR;
● 支持多相机同步/Multi−Camera Synchronization Support;
● 多款不同焦距镜头可选/Support different focal length lens;
[image: ]应用/Application
· 高级辅助驾驶和视觉融合/ADAS + Viewing Fusion
· 高动态应用/High Dynamic Range Imaging
[image: ]硬件框图/Hardware block diagram
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[image: ]关键参数/ KEY PARAMETERS
	序号
	Sensor参数
	OV OX08D10

	1
	Active Pixels(有效像素)
	8MP

	2
	Image Size(图像尺寸)
	1/1.73-inch CMOS

	3
	Shutter Type(曝光模式)
	Rolling Shutter 卷帘快门

	4
	Output Pixels(输出像素)
	3480*2160

	5
	Pixel Size(像素尺寸)
	2.1um*2.1um

	6
	ISP参数
	集成至Sensor

	7
	Frame Rate(帧率)
	30fps

	8
	Mirror(镜像)
	[bookmark: _GoBack]内置

	9
	Output data(输出信号格式)
	RAW

	10
	Lens参数
	近距:LC-C82-62A(信华)
	远距:LC-C82-64A(信华)

	11
	Lens Type(镜头结构)
	7G1GM
	8G

	12
	F/No.
	1.6±5%
	1.6±5%

	13
	E.F.L
	4.02±5%
	15.24±5%

	14
	F.O.V(Horizontal/Vertical)
	H:120.2°±2°
V:65.6°±1°
	H:29.9°±3°
V:17.0°±3°

	15
	OP Distortion(OP畸变)
	-58.6±5%
	<-1.31%@φ9.25

	16
	Relative Illumination(相对照度)
	70±5% 
	>70%@φ9.25

	17
	Focusing Distance
(调焦距离，物距)
	500mm(按应用的物距)

	18
	Depth of Field(景深范围)
	广角：≥3m
窄角：≥35m

	19
	整体模组
	参数

	20
	Dimensions(尺寸)
	L: 25mm, W:25mm, H:53mm(近距)
L: 25mm, W:25mm, H:58mm(远距)

	21
	Weight(重量)
	<50g

	22
	Connector(连接器)
	电连-818E92002Z

	23
	Serializer(串行器)
	MAXIM MAX96717F

	24
	Power Supply(工作电压)
	DC 12V

	25
	Current(工作电流)
	<250mA

	26
	Camera Interface(摄像头接口)
	LVDS

	27
	Optical Axis Precision
(光轴精度)
	X: ±5 Pixel，Y: ±5 Pixel

	28
	Startup Time(启动时间)
	<500ms

	29
	Operating temperature
(工作温度)
	-40℃~85℃

	30
	Storage temperature
(存储温度)
	-40℃~95℃

	31
	IP Grade(防护等级)
	模组本体IP52

	32
	MTF(清晰度)
	中心视场 MTF50P>0.7
0.7 视场 MTF50P>0.55(待实测)

	33
	Low Light(最低照度)
	1Lux

	34
	SNR(信噪比)
	44dB

	35
	HDR Range(动态范围)
	140 dB HDR4 (DCG + LOFIC + VS)

	36
	固件点亮配置
	参数

	37
	VSYNC极性
	TBD

	38
	主从模式
	Slave

	39
	数据有效位
	低8位

	40
	I2C地址
	0X6C

	41
	点亮配置
	TBD



附件Ⅰ：摄像头本体尺寸示意图(单位：mm)
	近距
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	远距
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